

**SODIUM CHLORIDE (NaCl) AEROSOL TEST**

(Aerosolized particles with a mass median diameter of approximately 0.26µm)

|  |  |
| --- | --- |
| COMPANY: |       |
| CONTACT: |       |
| LAB NUMBER/SAMPLE ID: |       |

TEST FLOW RATE: (available 0 to 100 L/min)

[ ]  85 ± 4 L/min (NIOSH/ASTM F3502 Parameters) [ ]  32 ± 2 L/min [ ]  28.3 L/min (Imitation of PFE)

[ ] \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

CONDITIONING: (**NIOSH = temp**: 38 ± 2.5º C, **relative humidity**: 85 ± 5%, **duration**: 25 ± 1 hour)

[ ]  YES (NIOSH/ASTM F3502 Parameters) [ ]  NO

TEST TYPE: (Please choose only one per Sample type)

[ ]  ASTM F3502 (Barrier Face Covering) [ ]  Instantaneous (~10 sec. FILTER Test)

[ ]  Initial Penetration (~1 min load)

[ ]  Max Penetration [ ]  Load Testing ( mg)

SAMPLE TEST SIDE: (Side that will be contacted by NaCl first):

[ ]  Outside (NIOSH Parameters, ASTM F3502) [ ]  Inside (Imitation of PFE) [ ]  \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

COMMENTS:

|  |  |  |  |
| --- | --- | --- | --- |
| SIGNATURE: |  | DATE: |  |

Confidential and Proprietary Information. Do not duplicate or copy.